Meeting @ The Foundry

|  |  |
| --- | --- |
| Member | Present |
| Brooke | ✓ |
| Henry | ✓ |
| Garrett | ✓ |
| Tamra | ✓ |
| Raiyan | ✓ |
| Jihan | ✓ |
| Edward | ✓ |

Troubleshooting

* Confirmed that the servos need to powered separately (not enough amps from the computer)
* Use oscilloscope to confirm that the signal wire actually gave out signal
* Confirmed that the BEC is unreliable
  + Now using a benchtop power supply to give the board what it wants
* Uploading the RC\_MIMIC code momentarily worked
  + Subsequently 5 beep error occurred

